Technical Specifications

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Feature | Specified | Current | Comments | Updated |
| WS2812 Interface | Running on the MCU, neither Library or DMA/Peripheral specified | On MCU, 1 PWM/DMA Stream over one GPIO |  |  |
| WS2812 Channels | 4 | 1 | 9 in total, some axis have 2 LED Rings |  |
| LED-Ring Animations | Not yet (quantity) | 2  Rainbow-like  Solid Color | The solid color is hard coded. |  |
|  |  |  |  |  |
| 1-Wire Master | Over 1 pin, running on the MCU (no external IC) | Direct communication over 1 pin, NO MASTER | GPIO + Timer without slave addressing |  |
| BS18B20 Slave Channels | 10 | 1 only | 1 temperature sensor should be on board |  |
| SPI Devices | Master on the MCU | none | EtherCAT and IMU external boards |  |
| SPI Channels | 2 | none |  |  |
| PCB Prototype |  | In process |  |  |
| 1 UART Port available | - | none | It might be needed for debugging |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
| BISS-C Device\* | Running on the MCU | - | This is out of scope |  |
| Encoder Channels | 2\* | - | Pinout should be further investigated |  |

Number of pins



Important Pinout

